# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

######  KURO – Information for invitation to tender



**Product:**

**PE cable protection bend / R=1000**

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE cable protection bend 125 x 3,9 mm  |
|  |  | ca. 15° / Radius = 1000 mm / Colour: black |
|  |  | with integral ring seal socket / DIN 16876 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE cable protection bend 125 x 3,9 mm  |
|  |  | ca. 30° / Radius = 1000 mm / Colour: black |
|  |  | with integral ring seal socket / DIN 16876 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE cable protection bend 125 x 3,9 mm  |
|  |  | ca. 45° / Radius = 1000 mm / Colour: black |
|  |  | with integral ring seal socket / DIN 16876 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE cable protection bend 125 x 3,9 mm  |
|  |  | ca. 90° / Radius = 1000 mm / Colour: black |
|  |  | with integral ring seal socket / DIN 16876 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |