# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

######  KURO – Information for invitation to tender

**Product:**

# Nr

#### PE double sealing socket with 2 seal rings

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE double sealing socket with 2 inner rings |
|  |  | Colour: black 50 x 3,0 mm / length = 185 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE double sealing socket with 2 inner rings |
|  |  | Colour: black 63 x 2,2 mm / length = 220 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE double sealing socket with 2 inner rings |
|  |  | Colour: black 75 x 3,0 mm / length = 250 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE double sealing socket with 2 inner rings |
|  |  | Colour: black 90 x 4,0 mm / length = 250 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE double sealing socket with 2 inner rings |
|  |  | Colour: black 110 x 4,3 mm / length = 300 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

****

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE double sealing socket with 2 inner rings |
|  |  | Colour: black 125 x 4,9 mm / length = 245 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE double sealing socket with 2 inner rings |
|  |  | Colour: black 140 x 8,0 mm / length = 278 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE double sealing socket with 2 inner rings |
|  |  | Colour: black 160 x 6,2 mm / length = 266 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE double sealing socket with 2 inner rings |
|  |  | Colour: black 180 x 4,8 mm / length = 233 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE double sealing socket with 2 inner rings |
|  |  | Colour: black 200 x 6,2 mm / length = 288 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |