# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

###### KURO – Information for invitation to tender

**Ein Bild, das Rechteck, Reihe, parallel, Diagramm enthält.

Automatisch generierte BeschreibungProduct:**

#### PVC double sealing socket

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 50 x 1,8 mm / Length = 170 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 63 x 1,9 mm / Length = 180 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 63 x 3,0 mm / Length = 180 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 75 x 2,2 mm / Length = 185 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 75 x 3,6 mm / Length = 200 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

****

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 90 x 2,7 mm / Length = 210 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 110 x 3,2 mm / Length = 410 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 110 x 5,3 mm / Length = 365 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 125 x 3,2 mm / Length = 365 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 140 x 4,1 mm / Length = 405 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black 160 x 4,7 mm / Length = 380 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |