# KURO_Logo

######  KURO – Information for invitation to tender



**Product:**

#### PE bends for cable protection – flexible / pressure tight

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE flexible, pressure-tight cable protection bends |
|  |  | with ring seal socket and plain end / watertight |
|  |  | 50 x 6,0 mm / long up to 90° / length = 2000 mm |
|  |  | Colour: black |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE flexible, pressure-tight cable protection bends |
|  |  | with ring seal socket and plain end / watertight |
|  |  | 110 x 6,0 mm / short up to 45° / length = 1500 mm |
|  |  | Colour: black |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE flexible, pressure-tight cable protection bends |
|  |  | with ring seal socket and plain end / watertight |
|  |  | 110 x 6,0 mm / long up to 90° / length = 2000 mm |
|  |  | Colour: black |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |