# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

######  KURO – Information for invitation to tender

**Product:**

#### PE sealing cap with anchoring eye

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE sealing cap 46 – 50 mm / Colour: black |
|  |  | Material: PELD / for socket and plain end |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE sealing cap 99 – 105 mm / Colour: black |
|  |  | Material: PELD / for socket and plain end System KURO o glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE sealing cap 142 – 150 mm / Colour: black |
|  |  | Material: PELD / for socket and plain end System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |