# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

###### KURO – Information for invitation to tender



**Product:**

#### PE sealings for cable protection pipe

hinged, for installed cables,

with special inlay made of foam neps

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE sealings for cable protection pipe  Inside pipe diameter: 61 - 66 mm |
|  |  | Colour: black |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PE sealings for cable protection pipe  Inside pipe diameter: 65 - 75 mm |
|  |  | Colour: black |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  |  |  |
|  | Pos:....................... | PE sealings for cable protection pipe  Inside pipe diameter: 94 - 98 mm |
|  |  | Colour: black |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE sealings for cable protection pipe  Inside pipe diameter: 98 - 102 mm |
|  |  | Colour: black |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE sealings for cable protection pipe  Inside pipe diameter: 134 - 144 mm |
|  |  | Colour: black |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PE sealings for cable protection pipe  Inside pipe diameter: 148 - 158 mm |
|  |  | Colour: black |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Menge:............Stück EP: ....... GP: ........ |

