# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

######  KURO – Information for invitation to tender



**Product:**

#### PP double sealing socket with inner ring

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PP double sealing socket with 2 seal rings |
|  |  | Colour: black 250 x 8,0 mm / length = 400 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |