# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

###### KURO – Information for invitation to tender

**Product:**

# 

#### PP fitting

Execution: with nut, cage, O- and Grip-Ring

Until 16 bar water- und airtight

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PP fitting for PE tube (min. SDR 13,6 und 11)  Dimension tube: 40 mm |
|  |  | Colour: orange / transparent |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PP fitting for PE tube (min. SDR 13,6 und 11)  Dimension tube: 50 mm |
|  |  | Colour: orange / transparent |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  |  |  |
|  | Pos:....................... | PP fitting for PE tube (min. SDR 13,6 und 11)  Dimension tube: 63 mm |
|  |  | Colour: orange / transparent |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |