# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

######  KURO – Information for invitation to tender

 Werksnorm

**Product:**

#### PVC cable protection pipe with integral seal socket



Length: 6000 mm

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 50 x 1,8 x 6000 mm |
|  |  | with integral ring seal socket incl. Trelleborg DIN-Lock sealing ring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  |  |  |
|  | Pos:....................... | PVC Cable protection pipe 50 x 2,4 x 6000 mm |
|  |  | with integral ring seal socket incl. Trelleborg DIN-Lock sealing ring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 63 x 1,9 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg POWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  |  |  |
|  | Pos:....................... | PVC Cable protection pipe 63 x 3,0 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg POWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  |  | ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif |
|  | Pos:....................... | PVC Cable protection pipe 75 x 2,2 x 6000 mm |
|  |  | with integral ring seal socket incl. Trelleborg DIN-Lock sealing ring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  |  |  |
|  | Pos:....................... | PVC Cable protection pipe 75 x 3,6 x 6000 mm |
|  |  | with integral ring seal socket incl. Trelleborg DIN-Lock sealing ring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  | Pos:....................... | PVC Cable protection pipe 90 x 2,7 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg POWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  | Pos:....................... | PVC Cable protection pipe 90 x 4,3 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg POWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  | Pos:....................... | PVC Cable protection pipe 110 x 3,2 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg SEWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  | Pos:....................... | PVC Cable protection pipe 110 x 5,3 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg SEWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  |  |  |
|  | Pos:....................... | ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gifPVC Cable protection pipe 125 x 3,7 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg SEWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  | Pos:....................... | PVC Cable protection pipe 125 x 6,0 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg SEWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  | Pos:....................... | PVC Cable protection pipe 140 x 4,1 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg POWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  |  |  |
|  | Pos:....................... | PVC Cable protection pipe 140 x 6,7 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg POWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  |  |  |
|  | Pos:....................... | PVC Cable protection pipe 160 x 4,7 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg SEWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  |  |  |
|  | Pos:....................... | PVC Cable protection pipe 160 x 7,7 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg SEWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  |  |  |
|  |  |  |
|  | Pos:....................... | PVC Cable protection pipe 200 x 4,0 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg SEWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  | Pos:....................... | PVC Cable protection pipe 200 x 5,9 x 6000 mm |
|  |  | mit Steckmuffe inkl. Trelleborg SEWER-Lock Dichtring |
|  |  | PVC-U / lead-free / in accordance to DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

