# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

######  KURO – Information for invitation to tender

 Werksnorm

**Product:**

#### PVC Cable protection pipe

Length: 6000 mm

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  |  |  |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 50 x 1,8 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 50 x 2,4 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 63 x 1,9 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 63 x 3,0 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 75 x 2,2 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |



|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 75 x 3,6 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 85 x 2,5 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 90 x 2,7 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 90 x 4,3 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 106 x 3,2 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 110 x 3,2 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |



|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 110 x 5,3 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |
|  | Pos:....................... | PVC Cable protection pipe 125 x 3,7 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 125 x 6,0 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 126 x 3,0 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 140 x 4,1 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 140 x 6,7 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |



|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 160 x 4,7 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 160 x 7,7 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC Cable protection pipe 200 x 4,0 x 6000 mmwith solvent welded socket / PVC-U / without lead |
|  |  | gefertigt nach DIN 16873 |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de) |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |