
# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

###### KURO – Information for invitation to tender



**Product:**

#### PVC divisible socket

* Transition from split duct (H-profile)

to closed cable protection pipe


# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC divisible socket from PVC split duct |
|  |  | with H-profile to closed cable protection pipe |
|  |  | Colour: black / 110 x 3,2 mm / Length = 250 mm |
|  |  | System KURO o.glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC divisible socket from PVC split duct |
|  |  | with H-profile to closed cable protection pipe |
|  |  | Colour: black / 125 x 3,7 mm / Length = 250 mm |
|  |  | System KURO o.glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC divisible socket from PVC split duct |
|  |  | with H-profile to closed cable protection pipe |
|  |  | Colour: black / 140 x 4,1 mm / Length = 250 mm |
|  |  | System KURO o.glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC divisible socket from PVC split duct |
|  |  | with H-profile to closed cable protection pipe |
|  |  | Colour: black / 160 x 4,7 mm / Length = 270 mm |
|  |  | System KURO o.glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

Ein Bild, das Text, Messing, Klammer enthält.

Automatisch generierte Beschreibung****

Ein Bild, das Text, Messing, Klammer enthält.

Automatisch generierte Beschreibung

* Transition from split duct (H-profile)

to split duct (H-profile)

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC divisible socket to connect |
|  |  | from split duct to split duct/ Colour: black |
|  |  | 110 x 3,2 mm / Length = 250 mm |
|  |  | System KURO o.glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC divisible socket to connect |
|  |  | from split duct to split duct/ Colour: black |
|  |  | 125 x 3,7 mm / Length = 250 mm |
|  |  | System KURO o.glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC divisible socket to connect |
|  |  | from split duct to split duct/ Colour: black |
|  |  | 140 x 4,1 mm / Length = 250 mm |
|  |  | System KURO o.glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC divisible socket to connect |
|  |  | from split duct to split duct/ Colour: black |
|  |  | 160 x 4,7 mm / Length = 270 mm |
|  |  | System KURO o.glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Metres UP: ....... TP: ........ |

H:\Bilder\LOGO\Kunststoffe\Punkt_Kuro_Kunstst.gif