# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

###### KURO – Information for invitation to tender

Ein Bild, das Reihe, parallel, Rechteck, Diagramm enthält.

Automatisch generierte Beschreibung**Product:**

#### PVC double sealing socket with inner ring

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black110 x 3,2 mm / Length = 410 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black110 x 5,3 mm / Length = 457 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black125 x 3,7 mm / Length = 365 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black125 x 6,0 mm / Length = 365 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sealing socket with 2 seal rings |
|  |  | Colour: black160 x 4,7 mm / Length = 380 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de), |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |