# ..\..\Bilder\LOGO\Kunststoffe\KURO_Logo.gif

######  KURO – Information for invitation to tender

**Product:**

#### PVC double sockets for adhesive jointing

# Information for invitation to tender:

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black50 x 1,8 mm / Length = 123 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black63 x 1,9 mm / Length = 144 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black63 x 3,0 mm / Length = 152 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black75 x 2,2 mm / Length = 165 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black75 x 3,6 mm / Length = 177 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

****

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black85 x 2,5 mm / Length = 185 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black90 x 2,7 mm / Length = 190 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black90 x 4,3 mm / Length = 202 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black106 x 3,0 mm / Length = 225 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black110 x 3,2 mm / Length = 270 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black110 x 5,3 mm / Length = 240 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black125 x 3,7 mm / Length = 285 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |



|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black125 x 6,0 mm / Length = 270 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black126 x 3,0 mm / Length = 265 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black140 x 4,1 mm / Length = 270 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black140 x 6,7 mm / Length = 288 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black160 x 4,7 mm / Length = 297 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black160 x 7,7 mm / Length = 315 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |



|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black200 x 4,0 mm / Length = 380 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |

|  |  |  |
| --- | --- | --- |
|  | Pos:....................... | PVC double sockets for adhesive jointing with DIN 16873 |
|  |  | Colour: black200 x 5,9 mm / Length = 280 mm |
|  |  | System KURO o. glw. (www.kuro-kunststoffe.de),  |
|  |  | supply and install, as an addition to pos: ........... |
|  |  |  |
|  |  | Amount:............Pieces UP: ....... TP: ........ |